



To reduce the loss 0.245 we go for back propogation

We have to update the weights and bias to make y^ and y equal

One forward propogation and calculation of loss function and decreasing that loss by using back propagation is 1 iteration this process goes continues untill y and y^ are equal

Optimisers are used in back propogation to reduce the loss function value



